# iVMS-4500 Help

1. Software Registration and Login
2. Live Preview
3. Device Management
4. Favorites
5. Channel Configuration
6. Local Config
7. Account Setting
8. Picture

# 1. Software Registration and Login

User need to register an administrator if this application is used for the first time, enter the user name and password in the register interface, and then click 'Register' to complete user registration.
If it's not the first time to run this application, the user name that used last time will be the default user name, before login, you also can enable 'Auto Login' to ignore the login process.

iVMS-4500 Help

# 2. Live Preview

Enter live preview interface by clicking 'Live Preview' in main menu, there is 4-split mode in default.
At the bottom of screen you can find some function buttons:
The definition of buttons from left to right are in the sequence of 'Stop', 'Bookmark', 'Quality', 'Capture', 'PTZ control'. 'Stop' button is used for stopping playing the selected camera, 'Bookmark' is used for saving the cameras now previewing, 'Quality' is used for adjust the quality of image, 'Capture' button is used for picture captured when in live preview. 'PTZ control' is used for enable or disable ptz ability. the pan and tilt control buttons are located in live preview interface:
click 'presets' button you will call out presets management panel; click 'bright' button you will call out bright management panel;
Swipe gesture can control up, down, left, right; Pinch gesture can control zoom in, zoom out.
Rotate iphone to landscape, image switch to full screen automatic, tap screen to show or hide toolbar.

iVMS-4500 Help

# 3. Device Management

After login successfully, the device list is empty in default. So firstly you need to add device, then all operations such as preview, configuration and device management can be available.
Click 'Devices' icon in the main menu to enter devices management interface, click 'Add' to go to new device added interface. You can select either 'IP' or 'DDNS' register mode to log on to the device, the new added device is in device management interface after you back.
Select a device in the list, click to modify the device information.
you can swipe on device, then popup the "Delete", click it to delete device.

iVMS-4500 Help

# 4. Favorites

Favorites is a function that manage the channels and bookmarks that makes the preview easier when only concern some specific cameras.
Click and navigate to 'Channels'->'Add' to go to favorites interface. Click the device to unfold the cameras list, you can add any of the cameras to your favorites by selecting it and then clicking 'Confirm' button.
Click and navigate to 'Bookmarks', can delete the bookmarks by swipe gesture.

iVMS-4500 Help

# 5. Channel Config

Click 'Channel Config' icon in main menu to enter channels configuration interface, all of the added devices are listed here.
Select the camera that needs to be configured, after logining successfully, enter parameters configuration interface, it's allowed to configure stream type, resolution, bit rate and frame rate, after finish the parameters adjustment, click 'Save' to complete the settings.
The parameters type can be 'Customize' or 'General', if select 'Customize', then all of parameters are configurable, or the channel parameters could not be adjusted.

iVMS-4500 Help

# 6. Local Config

You can enter local configuration interface by clicking 'LocalConfig' icon in main menu, In the PTZ step option, you can drag the slider to adjust the speed in pan and tilt direction, there are seven steps in all.

iVMS-4500 Help

# 7. Account Setting

In the 'AccountSetting' sub menu, you are allowed to modify your current password. Enter old password, new password and then confirm new password to complete the modification.

iVMS-4500 Help

# 8. Picture

To find picture snapshoted, please enter "Photos" application.

iVMS-4500 Help

#